{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":8,"n_cols":10,"rows_kept":8,"merged":[[0,4,0,9]],"flags":["formulas_cached_only"]}
["Fixed-point MP3 average CPU usage","Sample Rate","Bit Rate","Channels","Processor Model"]
["/datatype/mp3/codec/fixpt - 08/05/03",{"$nulls":3},"ARM7TDMI","ARM9TDMI-REV2","ARM920T","ARM9E","StrongARM1","XScale"]
[null,48000,"320 kbps",2,"30 MHz","24 MHz","27 MHz","20 MHz","20 MHz","20 MHz"]
["Notes:",44100,"128 kbps",2,"26 MHz","21 MHz","24 MHz","17 MHz","17 MHz","17 MHz"]
["* Numbers are from ARMulator, simulated"]
["      zero-wait state memory"]
["* Compiled using ARM ADS 1.2 with"]
["      appropriate target CPU"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}