{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":40,"n_cols":2,"rows_kept":40,"flags":["formulas_cached_only"]}
["Fixed-point MP3 memory usage"]
["/datatype/mp3/codec/fixpt - 08/05/03"]
[]
["Notes:"]
["* Memory usage constant for all sample rates, bit rates"]
["* Does not include input buffer (encoded data)"]
["      or output buffer (PCM)"]
["* There is no zero-init or read-write global data"]
["* Some compilers (like ADS) might put small ROM"]
["      tables in code (.text) section, so expect small"]
["      variations in code/data size depending on compiler"]
[]
["All values are in bytes"]
[]
["ROM (const globals)"]
["mp3tabs.obj",1290]
["dct32.obj",192]
["dqchan.obj",592]
["hufftabs.obj",8968]
["imdct.obj",144]
["scalfact.obj",104]
["trigtabs.obj",2156]
["ROM Total",13446]
[]
["RAM (heap)"]
["MP3DecInfo",2032]
["FrameHeader",56]
["SideInfo",328]
["ScaleFactorInfo",284]
["HuffmanInfo",4624]
["DequantInfo",840]
["IMDCTInfo",6944]
["SubbandInfo",8708]
["RAM Total",23816]
[]
["Total Data Memory (ROM + RAM)",37262]
[]
["Code size - x86 (MSVC++ 6.0)",28288]
["Code size - ARM (ADS ARM9TDMI)",20744]
[" (these sizes vary with compiler settings, etc.)"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}